{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Tabelle1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Tabelle1","index":0,"n_rows":16,"n_cols":4,"rows_kept":16,"cut":false,"hidden":false,"merged":[]}
["Pin ","GPIO",null,"Regler"]
[2,"5v",null,"VCC"]
[6,"GND",null,"GND"]
[8,"GPIO 14",null,"In1"]
[10,"GPIO 15",null,"In2"]
[12,"GPIO 18",null,"In3"]
[16,"GPIO 23",null,"In4"]
[18,"GPIO 24",null,"In5"]
[22,"GPIO 25",null,"In6"]
[24,"GPIO 8",null,"In7"]
[26,"GPIO 7",null,"In8"]
[]
[]
["GPIO -g mode 14 out"]
["gpio -g write 14 1"]
["gpio -g write 14 0"]